commit f2c679d4b2c73a95f437c705f960a4af1fa23498
Author: H.J. Lu <hjl.tools@gmail.com>
Date:   Tue Sep 15 05:49:27 2020 -0700

    <sys/platform/x86.h>: Add Intel Key Locker support
    
    Add Intel Key Locker:
    
    https://software.intel.com/content/www/us/en/develop/download/intel-key-locker-specification.html
    
    support to <sys/platform/x86.h>.  Intel Key Locker has
    
    1. KL: AES Key Locker instructions.
    2. WIDE_KL: AES wide Key Locker instructions.
    3. AESKLE: AES Key Locker instructions are enabled by OS.
    
    Applications should use
    
    if (CPU_FEATURE_USABLE (KL))
    
    and
    
    if (CPU_FEATURE_USABLE (WIDE_KL))
    
    to check if AES Key Locker instructions and AES wide Key Locker
    instructions are usable.

diff --git a/manual/platform.texi b/manual/platform.texi
index 2c145acdc3564cbb..95b0ed0642c9f8a9 100644
--- a/manual/platform.texi
+++ b/manual/platform.texi
@@ -177,6 +177,9 @@ The supported processor features are:
 @item
 @code{AES} -- The AES instruction extensions.
 
+@item
+@code{AESKLE} -- AES Key Locker instructions are enabled by OS.
+
 @item
 @code{AMX_BF16} -- Tile computational operations on bfloat16 numbers.
 
@@ -353,6 +356,9 @@ the indirect branch predictor barrier (IBPB).
 @item
 @code{INVPCID} -- INVPCID instruction.
 
+@item
+@code{KL} -- AES Key Locker instructions.
+
 @item
 @code{L1D_FLUSH} -- IA32_FLUSH_CMD MSR.
 
@@ -598,6 +604,9 @@ using a TSC deadline value.
 @item
 @code{WBNOINVD} -- WBINVD/WBNOINVD instructions.
 
+@item
+@code{WIDE_KL} -- AES wide Key Locker instructions.
+
 @item
 @code{X2APIC} -- x2APIC.
 
diff --git a/sysdeps/x86/cpu-features.c b/sysdeps/x86/cpu-features.c
index 6954728c47d0126b..77a596a15404b575 100644
--- a/sysdeps/x86/cpu-features.c
+++ b/sysdeps/x86/cpu-features.c
@@ -269,6 +269,14 @@ update_usable (struct cpu_features *cpu_features)
   /* Determine if PKU is usable.  */
   if (CPU_FEATURES_CPU_P (cpu_features, OSPKE))
     CPU_FEATURE_SET (cpu_features, PKU);
+
+  /* Determine if Key Locker instructions are usable.  */
+  if (CPU_FEATURES_CPU_P (cpu_features, AESKLE))
+    {
+      CPU_FEATURE_SET (cpu_features, AESKLE);
+      CPU_FEATURE_SET_USABLE (cpu_features, KL);
+      CPU_FEATURE_SET_USABLE (cpu_features, WIDE_KL);
+    }
 }
 
 static void
@@ -341,6 +349,12 @@ get_common_indices (struct cpu_features *cpu_features,
 		   cpu_features->features[COMMON_CPUID_INDEX_D_ECX_1].cpuid.ecx,
 		   cpu_features->features[COMMON_CPUID_INDEX_D_ECX_1].cpuid.edx);
 
+  if (cpu_features->basic.max_cpuid >= 0x19)
+    __cpuid_count (0x19, 0,
+		   cpu_features->features[COMMON_CPUID_INDEX_19].cpuid.eax,
+		   cpu_features->features[COMMON_CPUID_INDEX_19].cpuid.ebx,
+		   cpu_features->features[COMMON_CPUID_INDEX_19].cpuid.ecx,
+		   cpu_features->features[COMMON_CPUID_INDEX_19].cpuid.edx);
 }
 
 _Static_assert (((index_arch_Fast_Unaligned_Load
diff --git a/sysdeps/x86/sys/platform/x86.h b/sysdeps/x86/sys/platform/x86.h
index ebc5f6fc16cb8104..bcc81ab5f8ac8265 100644
--- a/sysdeps/x86/sys/platform/x86.h
+++ b/sysdeps/x86/sys/platform/x86.h
@@ -28,6 +28,7 @@ enum
   COMMON_CPUID_INDEX_80000007,
   COMMON_CPUID_INDEX_80000008,
   COMMON_CPUID_INDEX_7_ECX_1,
+  COMMON_CPUID_INDEX_19,
   /* Keep the following line at the end.  */
   COMMON_CPUID_INDEX_MAX
 };
@@ -224,7 +225,7 @@ extern const struct cpu_features *__x86_get_cpu_features (unsigned int)
 /* Note: Bits 17-21: The value of MAWAU used by the BNDLDX and BNDSTX
    instructions in 64-bit mode.  */
 #define bit_cpu_RDPID		(1u << 22)
-#define bit_cpu_INDEX_7_ECX_23	(1u << 23)
+#define bit_cpu_KL		(1u << 23)
 #define bit_cpu_INDEX_7_ECX_24	(1u << 24)
 #define bit_cpu_CLDEMOTE	(1u << 25)
 #define bit_cpu_INDEX_7_ECX_26	(1u << 26)
@@ -312,6 +313,12 @@ extern const struct cpu_features *__x86_get_cpu_features (unsigned int)
 /* EAX.  */
 #define bit_cpu_AVX512_BF16	(1u << 5)
 
+/* COMMON_CPUID_INDEX_19.  */
+
+/* EBX.  */
+#define bit_cpu_AESKLE		(1u << 0)
+#define bit_cpu_WIDE_KL		(1u << 2)
+
 /* COMMON_CPUID_INDEX_1.  */
 
 /* ECX.  */
@@ -437,7 +444,7 @@ extern const struct cpu_features *__x86_get_cpu_features (unsigned int)
 #define index_cpu_INDEX_7_ECX_15 COMMON_CPUID_INDEX_7
 #define index_cpu_INDEX_7_ECX_16 COMMON_CPUID_INDEX_7
 #define index_cpu_RDPID		COMMON_CPUID_INDEX_7
-#define index_cpu_INDEX_7_ECX_23 COMMON_CPUID_INDEX_7
+#define index_cpu_KL		COMMON_CPUID_INDEX_7
 #define index_cpu_INDEX_7_ECX_24 COMMON_CPUID_INDEX_7
 #define index_cpu_CLDEMOTE	COMMON_CPUID_INDEX_7
 #define index_cpu_INDEX_7_ECX_26 COMMON_CPUID_INDEX_7
@@ -525,6 +532,12 @@ extern const struct cpu_features *__x86_get_cpu_features (unsigned int)
 /* EAX.  */
 #define index_cpu_AVX512_BF16	COMMON_CPUID_INDEX_7_ECX_1
 
+/* COMMON_CPUID_INDEX_19.  */
+
+/* EBX.  */
+#define index_cpu_AESKLE	COMMON_CPUID_INDEX_19
+#define index_cpu_WIDE_KL	COMMON_CPUID_INDEX_19
+
 /* COMMON_CPUID_INDEX_1.  */
 
 /* ECX.  */
@@ -650,7 +663,7 @@ extern const struct cpu_features *__x86_get_cpu_features (unsigned int)
 #define reg_INDEX_7_ECX_15	ecx
 #define reg_INDEX_7_ECX_16	ecx
 #define reg_RDPID		ecx
-#define reg_INDEX_7_ECX_23	ecx
+#define reg_KL			ecx
 #define reg_INDEX_7_ECX_24	ecx
 #define reg_CLDEMOTE		ecx
 #define reg_INDEX_7_ECX_26	ecx
@@ -738,4 +751,10 @@ extern const struct cpu_features *__x86_get_cpu_features (unsigned int)
 /* EAX.  */
 #define reg_AVX512_BF16		eax
 
+/* COMMON_CPUID_INDEX_19.  */
+
+/* EBX.  */
+#define reg_AESKLE		ebx
+#define reg_WIDE_KL		ebx
+
 #endif  /* _SYS_PLATFORM_X86_H */
diff --git a/sysdeps/x86/tst-get-cpu-features.c b/sysdeps/x86/tst-get-cpu-features.c
index 95e0d33f6c7eeace..c01d701b52090983 100644
--- a/sysdeps/x86/tst-get-cpu-features.c
+++ b/sysdeps/x86/tst-get-cpu-features.c
@@ -170,6 +170,7 @@ do_test (void)
   CHECK_CPU_FEATURE (AVX512_BITALG);
   CHECK_CPU_FEATURE (AVX512_VPOPCNTDQ);
   CHECK_CPU_FEATURE (RDPID);
+  CHECK_CPU_FEATURE (KL);
   CHECK_CPU_FEATURE (CLDEMOTE);
   CHECK_CPU_FEATURE (MOVDIRI);
   CHECK_CPU_FEATURE (MOVDIR64B);
@@ -217,6 +218,8 @@ do_test (void)
   CHECK_CPU_FEATURE (INVARIANT_TSC);
   CHECK_CPU_FEATURE (WBNOINVD);
   CHECK_CPU_FEATURE (AVX512_BF16);
+  CHECK_CPU_FEATURE (AESKLE);
+  CHECK_CPU_FEATURE (WIDE_KL);
 
   printf ("Usable CPU features:\n");
   CHECK_CPU_FEATURE_USABLE (SSE3);
@@ -323,6 +326,7 @@ do_test (void)
   CHECK_CPU_FEATURE_USABLE (AVX512_BITALG);
   CHECK_CPU_FEATURE_USABLE (AVX512_VPOPCNTDQ);
   CHECK_CPU_FEATURE_USABLE (RDPID);
+  CHECK_CPU_FEATURE_USABLE (KL);
   CHECK_CPU_FEATURE_USABLE (CLDEMOTE);
   CHECK_CPU_FEATURE_USABLE (MOVDIRI);
   CHECK_CPU_FEATURE_USABLE (MOVDIR64B);
@@ -370,6 +374,8 @@ do_test (void)
   CHECK_CPU_FEATURE_USABLE (INVARIANT_TSC);
   CHECK_CPU_FEATURE_USABLE (WBNOINVD);
   CHECK_CPU_FEATURE_USABLE (AVX512_BF16);
+  CHECK_CPU_FEATURE_USABLE (AESKLE);
+  CHECK_CPU_FEATURE_USABLE (WIDE_KL);
 
   return 0;
 }
