From 25251c0707fe34f30a27381a5fabc35435a96621 Mon Sep 17 00:00:00 2001
From: Stefan Liebler <stli@linux.ibm.com>
Date: Tue, 16 Feb 2021 16:18:56 +0100
Subject: [PATCH] S390: Add new hwcap values.

The new hwcap values indicate support for arch14 architecture.
---
 sysdeps/s390/dl-procinfo.c                | 5 +++--
 sysdeps/s390/dl-procinfo.h                | 4 +++-
 sysdeps/unix/sysv/linux/s390/bits/hwcap.h | 2 ++
 3 files changed, 8 insertions(+), 3 deletions(-)

diff --git a/sysdeps/s390/dl-procinfo.c b/sysdeps/s390/dl-procinfo.c
index 0c334a2551..c174e27b35 100644
--- a/sysdeps/s390/dl-procinfo.c
+++ b/sysdeps/s390/dl-procinfo.c
@@ -46,12 +46,13 @@
 #if !defined PROCINFO_DECL && defined SHARED
   ._dl_s390_cap_flags
 #else
-PROCINFO_CLASS const char _dl_s390_cap_flags[19][9]
+PROCINFO_CLASS const char _dl_s390_cap_flags[21][9]
 #endif
 #ifndef PROCINFO_DECL
 = {
      "esan3", "zarch", "stfle", "msa", "ldisp", "eimm", "dfp", "edat", "etf3eh",
-     "highgprs", "te", "vx", "vxd", "vxe", "gs", "vxe2", "vxp", "sort", "dflt"
+     "highgprs", "te", "vx", "vxd", "vxe", "gs", "vxe2", "vxp", "sort", "dflt",
+     "vxp2", "nnpa"
   }
 #endif
 #if !defined SHARED || defined PROCINFO_DECL
diff --git a/sysdeps/s390/dl-procinfo.h b/sysdeps/s390/dl-procinfo.h
index 9e1a8c7ba9..2d9c305808 100644
--- a/sysdeps/s390/dl-procinfo.h
+++ b/sysdeps/s390/dl-procinfo.h
@@ -21,7 +21,7 @@
 #define _DL_PROCINFO_H	1
 #include <ldsodefs.h>
 
-#define _DL_HWCAP_COUNT 19
+#define _DL_HWCAP_COUNT 21
 
 #define _DL_PLATFORMS_COUNT	10
 
@@ -61,6 +61,8 @@ enum
   HWCAP_S390_VXRS_PDE = 1 << 16,
   HWCAP_S390_SORT = 1 << 17,
   HWCAP_S390_DFLT = 1 << 18,
+  HWCAP_S390_VXRS_PDE2 = 1 << 19,
+  HWCAP_S390_NNPA = 1 << 20,
 };
 
 #define HWCAP_IMPORTANT (HWCAP_S390_ZARCH | HWCAP_S390_LDISP \
diff --git a/sysdeps/unix/sysv/linux/s390/bits/hwcap.h b/sysdeps/unix/sysv/linux/s390/bits/hwcap.h
index 696616e779..e9bd3684db 100644
--- a/sysdeps/unix/sysv/linux/s390/bits/hwcap.h
+++ b/sysdeps/unix/sysv/linux/s390/bits/hwcap.h
@@ -46,3 +46,5 @@
 #define HWCAP_S390_VXRS_PDE     65536
 #define HWCAP_S390_SORT         131072
 #define HWCAP_S390_DFLT         262144
+#define HWCAP_S390_VXRS_PDE2    524288
+#define HWCAP_S390_NNPA         1048576
-- 
2.31.1

